# 测试员的自我评价(七篇)

来源：网络 作者：九曲桥畔 更新时间：2024-10-02

*在日常的学习、工作、生活中，肯定对各类范文都很熟悉吧。范文书写有哪些要求呢？我们怎样才能写好一篇范文呢？这里我整理了一些优秀的范文，希望对大家有所帮助，下面我们就来了解一下吧。测试员的自我评价篇一i remember the first w...*

在日常的学习、工作、生活中，肯定对各类范文都很熟悉吧。范文书写有哪些要求呢？我们怎样才能写好一篇范文呢？这里我整理了一些优秀的范文，希望对大家有所帮助，下面我们就来了解一下吧。

**测试员的自我评价篇一**

i remember the first week of internship, we are very excited, a week down we feel very relaxed, rest for two days, began measuring practice, i followed the teacher to find the control point, then everyone is still excited, that the next of the week should also be very easy, it is gh a bit lucky, but we all learn a lot, only a lot of ordinary \"a lot of shopping\" to learn things. i like to think, like the summary, so i summed up the following points:

grow up, to try to take some responsibility. we are born with a kind of inertia, whether inspaniduals, or a team, if it is in an inert atmosphere, that she (people) efficiency will not be high, but if everyone has a strong sense of responsibility, take some responsibility, then the efficiency is not only improved, and the task will be completed very well.

infectivity is very important. in a team, in order to have a good atmosphere, the first person to put forward the idea of thinking is very important, because later people can not help but have a herd mentality. if he (she) the idea is positive, then someone will actively think of some problems. on the contrary, the whole team into a negative atmosphere. therefore, each of us should actively think about the problem.

think a lot. what is the internship, internship is the theoretical knowledge into their own knowledge of the process. internship process only a lot of thinking, in order to digest a lot of knowledge, but also extends a lot of previously unknown. teamwork, through thick and thin. this is a cliché, but in this practice have to mention, because it is everywhere, remember very clearly that many times we are on the measurement site for lunch; is that we all get up early, and then in the cold whiz in the operation, everyone in the trembling; we are carrying the instrument touched the black home. all this bitter and happy, we all bear together. through thick and thin, we are happy! learn to compromise. compromise is the highest art, in the process of cooperation, inevitably there will be some conflicts, then we need to calm down to think about the solution to the problem, everyone has done some concessions, then things are easy to the most \"humble\" work, tree arrogant self-esteem. a good team, everyone needs a little hard work, not afraid of dirty, not afraid of tired, rather than pushing three or four. only everyone is actively doing everything, in order to achieve the purpose of the internship, so that everyone is familiar with every aspect.

to calm. whether doing things or a man, we should learn to calmly face. remember half of the picture, the teacher pointed out that we are wrong method of mapping, we have thought would be wrong; remember the distance with a tape measure we have thought about measuring only once. but in the end we did not do, now think of it, this is right! frankly, is what we want life.

internship is completed, the internship is the most unforgettable day of my life, very afraid of the beginning, and now want to come, the day is over, and can get good interns, so get a revelation: no matter what difficulties,do not lose confidence in yourself.

**测试员的自我评价篇二**

time off quickly, blink of an eye, i went to hengyuan company project department, has more than six these days, success, failure, joy, and distress. in the leadership of the care and guidance, colleagues in the full support and help, my ability to work has been greatly improved.

from the unit, i know their own shortcomings and the direction of the effort, now in the project department engaged in the measurement of construction tests and so on. in addition to the work of the ministry of construction, , to learn more about my colleagues work knowledge and communication. i know that their experience and experience are inadequate, practice is also very flawed, but do not know i asked, and access to information and drawings, colleagues in the office and the leadership of the help, feel that they learned these days many, every day is full. now the work of these days to do a self-assessment.

1, 1, to study hard and continuously improve professional competence. at work, serious study of professional knowledge, practice and theory will be combined, continue to accumulate experience, a lot of professionals, technical staff advice, and constantly enrich themselves;

2, abide by the rules and regulations, these days, their work is not afraid of hardship, not afraid of tired, learning excellent staff approach, more to see more to listen to more questions, carefully to complete the construction test of the work tasks; , unity of colleagues, work together, colleagues, harmonious relations, unity and fraternity, mutual help, mutual respect and understanding;

4, due to their lack of work experience in the work of the lack of practical experience, quality inspection work done inadequate, through the subsequent accumulation of learning and practice, and more to my colleagues to learn, this is my future work to make good efforts direction.

second, the attitude in the professional, everyone has a motivated heart, i not only work for the company, working for the boss, i work for themselves, i believe they can do a very hot heart, a pair of very hard - working hands. on the one hand i should not rigidly adhere to some things, to be good at breakthroughs, creative ideas, but also to the overall situation, the team as the most important, can not be too personal. and then later in the process of doing things to pay attention to the method, so as to make work more efficient and reduce unnecessary duplication of work, things will do better. in the professional field, i have been working in the project department of the company. with the help of my colleagues, i have gained more and more knowledge through professional efforts and work experience.

3, review these days, i seriously study the professional knowledge of road and bridge, study diligently, wholeheartedly, courteous, warm, patiently answer the problems in the work, and in practice to improve their quality and professional level, and strive to grow as a qualified hengyuan employees. these days, let me on their own jobs and the company\'s advantages of resources, have a more profound understanding and understanding, which can be more quickly adapt to their jobs, give full play to their initiative, in the future work andlife, i believe that through their own efforts, in the future work, i will grow into a professional and responsible staff, to become the object of learning for others to contribute to the company. with the increase in their working days, to achieve their goals, reflecting the value of their lives, and the company grow together. i will use modest attitude and full of enthusiasm to do my job, create value for the company, with the company to look forward to a better future!

**测试员的自我评价篇三**

blink of an eye 10 years have gone, we ushered in a new year. summing up the work of the past year, from a personal point of view about the measurement of awareness.

quality is the life, quality is the fundamental guarantee for enterprise development. in the fierce competition in the construction market today, how to improve the construction quality management level is every enterprise managers must think about. factors affecting the quality of construction in all aspects. from the engineering measurement point of view, analyze the work of measuring the pay-off to ensure and improve the quality of the construction of an important role, and simply how to strengthen the management of measurement work to improve the quality of construction.

it is a very important technical work of municipal road engineering that the measuring and measuring line is an important technical work. it is inseparable from the whole process of construction, from the preparation before construction to the completion of the construction, to the final acceptance after construction. how to do a quick and good measurement of the line, is a basic technical skills and test the basic requirements.

do the measurement before the commencement of the end

before the start of the project, the survey and design units shall be responsible for on-site surveying and settlement according to the design documents, and the site standard point, conductor piles and crossing point piles shall be clearly identified according to the design drawings. within the measurement of signs, must take appropriate protection measures. on the measurement of the end, it is necessary to emphasize the protection of pile position, that is, in the design unit after pile, should be timely use of brick piers or pouring cement pier and other methods to be protected, so as not to lose. these piles are generally farmland or residential areas, it is easy to be man-made destruction, and once destroyed, let the survey and design units to fill test, then delay the construction, but also increase the cost.

midline retest and edge loft

center line measurement is based on the alignment measurement, the road center line plane position on the ground marked in detail. it is the difference with the alignment measurement is: alignment measurement, but the intersection of the road and the straight line segment of the necessary turning point marked out, and in the midline measurement, according to the intersection and the turning point with a series of stakes will road straight segment and curve segments are specified in detail on the ground.

the alignment survey is usually carried out by the survey and design units, and then the pile and measurement results to the construction side, the construction unit by the middle line and construction measurement.

subgrade construction should be fully restored before the center line, according to the restoration of the pile in the road and the relevant provisions of the roadbed side of the pile. on the midline re-measurement and edge lofting, should pay attention to the following points;

one should pay attention to the distance between the intersection, the direction is consistent with the drawings; such as an engineering project has several tenders, should pay attention to the center of the adjacent tenders are closed, midline measurements should be in-depth adjacent tenders 50 ~ 100 m; attention should be paid to the center of the structure such as bridge and culvert is closed; should pay attention to the relative position of the building and other buildings and drawings are consistent. if you find problems in a timely manner to identify the reasons for the design unit.

second, retaining pile set. it is very important to set up pile protection pile in the middle of the road, but these piles are easy to be destroyed during the construction. therefore, it is necessary to carry out the restoration and surveying work of the middle pile during the construction of the roadbed. in order to quickly and accurately restore the center pile in the original position, must be on the road before the construction of the main control point of the pile such as the intersection point, turning point, curve control points set up retaining pile. the so-called retaining pile, is outside the scope of the construction is not easy to be destroyed where some stakes set ing to these pile, with simple methods (such as the intersection point, range, etc.), you can quickly restore the original pile point.

set the pile should pay attention to the following aspects: in each straight section of the road, at least three control piles to set up retaining pile, so even if there is a control pile can not be restored, the other two points can be used to restore the straight section to the original position; the intersection angle of the two direction lines as close as possible to 90 °, should not be less than 30 ° angle of intersection; retaining pile should be selected outside the scope of construction, but not too far away; pile distance can not be too far; the retaining pile must be solid and reliable, pile to facilitate the erection of measuring instruments and observation.

set up retaining pile of curve side. for the curve segment, because of the more difficult to determine the side of the pile, re-measuring time-consuming more, so after a precise line, the edge of the curve section of the pile pile should also be set representative pile, which can reduce repeat the measurement, reducing the measurement workload.

third, the laying of mileage pile. after the midline pile is fixed, it is possible to lay out the control pile of the mileage pile on this basis. mileage pile layout principle is: in the straight section, generally arranged in every 100 meters of the entire pile of cross-section, similar to the common road construction 100 meters pile layout; in the curve section of the pile to be properly encrypted, in the curve mileage pile can be large stakes, above the mileage mark with paint or ink station, into the road outside the scope of construction on both sides of the ground, it is best to play on each side of a . to ensure that the construction is not easy to damage the case, from the embankment edge should be as close as possible to facilitate the use, generally 1 to 2 meters.

the laying of mileage piles is not addressed in most of the surveying and setting-out sections of the construction manual, and is not taken into account at many sites. i found in some sites, some construction technicians in the construction survey, the determination of the distance station is a long distance from a foot a foot row over, not only a waste of time and prone to cumulative error. if the mileage stakes are not allowed, then the elevation, slope quality control is out of the question.

third, the proofreading and additional standard point

first, the use of design units set up before the standard point should be carefully checked, close the gap may not exceed the limit, such as exceeding the allowable deviation should identify the reasons and promptly reported to the relevant departments. the design unit delivers the leveling points normally set several months ago. these points in the field can easily be man-made collision or natural subsidence due to the ground changes, so be sure to carefully review before use; second, the standard point of additional principles: the distance is generally 150 to 200 meters, plus transfer station for the principle. the additional standard point should be closed with the design unit to pay the standard point, such as an engineering project at several tenders, but also with the adjacent standard segment of the standard point of closure, the closure may not exceed the limit.

the position of the leveling point shall be located on a solid, non-sinking, non-touching ground or a solid building of a permanent building. can also be installed in the protection of deep-buried wood piles or concrete piles, and make clear signs. the leveling point should be checked once a month, and the level of the spot where the movement is suspected should be checked after re-inspection.

vertical and horizontal cross-section measurement

through the midline re-test, side piles line and the laying of the standard point, you can measure the vertical and horizontal cross-section. the main purpose of vertical and horizontal cross-section measurement is to calculate the amount of earth, so the vertical and horizontal cross-section measurement after the end of the measurement results should be checked with the design drawings. where the results with the original within the allowable deviation, the original results shall prevail, and only when there are significant differences with the original results, can be reported to the supervisory engineer after verification changes. it should be noted that: the work must be carried out before construction. if the measured amount of earth and the design does not conform to the supervision of the approval should also be carried out before site excavation to the supervisor before the actual amount of earthwork and design does not match, require additional visa, but the final supervision be sure to pay attention to the timeliness of the work.

**测试员的自我评价篇四**

during this period to seriously comply with the rules and regulations of the new group, love plants such as love home, but also at work

constantly strict demands on themselves, with the ministry of the production process work, the layout of the leadership to complete the various tasks. diligent and enterprising, innovative, and continuously improve their work efficiency and found that the work of the problems in a timely manner to report to the leadership and seek solutions to the company\'s development and make greater contributions.

first, study with great concentration, conscious temper.

although i took the forklift driving license is not long, just started, the operation is not particularly skilled, but in the course of my study, and consciously temper. after 3 months, i have been able to carry out skilled operation control, posts for three months to basically no mistakes, the ability to work has been greatly improved. for the future to complete the work to lay a solid foundation. i will continue in the next work, to further improve my professional level, at the same time to do a better job.

second, strict requirements, love and respect their jobs.

work in strict demands on themselves, diligent, love and respect their jobs, do not bow before difficulties do not back in front of the work, high-quality completed the work. in future work, i will humbly ask experienced instructors, and constantly sum up experience, to make up for their own deficiencies. at the same time, continue to learn a variety of theoretical knowledge and professional skills for the company\'s contribution to the development of their own strength!

third, strengthen training, improve operational skills.

in order to do their work well, i make full use of limited time, strengthen the operation skills training, improve the efficiency of loading and unloading operations to ensure the safety of loading and unloading trucks, before the operation must be loaded with the number of pieces of goods, specifications for serious study to determine the code put standard, so as to ensure the volume filled with the vehicle. i remember the beginning of forklift operations, i have flip then, i have to strengthen all aspects of skills training, and achieved good results, summed up a set of forklift driver training methods.

**测试员的自我评价篇五**

our company development and production of hook-tail box, on the heart plate, support blocks and other new railway products, transferred from june

qc department after the initiative to help guide the leadership of new product debugging and production, will know and in the work should focus on issues and front-line staff one by one detailed, auxiliary production work carried out smoothly. in the independent sent to the machine shop, the timely and timely follow up the progress of each new product processing and the establishment of accounting, so that each new product from the machine into the workshop to start the process, each step real-time monitoring. timely detection and feedback of new products in the process of the existing problems and to assist the technology sector to improve the processing technology. and ensure the successful completion of mechanical processing of sample samples for crcc certification of \"forged steel upper plate for railway wagons\", \"13b forged coupler end frame\" and \"17 forged hooktail frame\".

◆ personal strengths and weaknesses

i learned mechanical manufacturing, and previously engaged in haier is mainly automated robotic aspects of testing, came after the company has only been working in the machine shop, the knowledge of the relatively lack of forging. when i first came to the qc department of the forging workshop, i almost did not know the company\'s forging products. after consulting with my colleagues, i quickly learned about the performance and key points of each product. . i am from the machine plus apprentices began to come step by step, mechanical processing, programming knowledge more solid. in the machine after the workshop, not only to ensure that machine products and timely detection, and can be found in the process of the hidden dangers, to avoid the occurrence of quality accidents, auxiliary site production. ◆ personal development goals in the company

quality inspection work is not a simple size detection. at present our departments involved: forging detection, machining finished product testing, tensile, impact test, metallographic test, hardness, magnetic detection, ultrasonic testing. debugging products related to bridge bearings, construction machinery, coal mining machinery, truck parts, etc., processes heating, forging, roll forging, heat treatment, machining, etc., these things are the wealth of the hands of the company in the detection sector is not to so many things. in future work, i will, as always, people: people with good, the work: to perfect, the quality: strict hold. and constantly strive to learn and expand their knowledge, assiduously enhance their business level to look forward to the development of the company to do their part.

◆ recommendations for the company

attention to detail, emotional trivia in life to increase points, in principle, equality and discrimination on the issue of everyone, improve employee sense of belonging and well-being, to retain talent to create a win-win situation. i listed below a few examples of qingdao haier mold co., ltd.: employee birthday, wedding anniversary, the birthday of the children and other commemorative date, timely delivery of small gifts or leave, pull the distance between the company and employees to improve staff members of the familysatisfaction and support.

**测试员的自我评价篇六**

time flies, a flash of the new semester is about to begin, and slowly away from us in 20xx, the first semester of university life is officially announced the end, but the year 20xx, which will always have our beautiful memories. this year we for our own goals, dreams, we cried we laughed, we also experienced the university of study and life, and here to get to know a lot of good students together, good friends, good brothers.

20xx was a very important and memorable year for me because there was a big change in my life both in my studies and in my life. university of the time day, week, month in the past, we met each other new students, together with military training, learning together, their choice of favorite associations. university life is very rich and very free, some people are busy, leisurely you can 24 hours at the computer game, but some people are busy, can be busy to the day without even the rest of time, i think the university has two kinds of people, play dead and busy dead people, in fact, this is like an endless ladder on both sides, we are beginning to set sail in the middle, forward and backward are in an idea. i like the latter, so tired though, but full.

recalling the freshman, i also have a lot of things to do in many ways is not good enough. in view of the lack of last semester, i feel we should try to start from the following aspects, and strive to do: 1 learning

(1) the study of specialized courses, should be clear objectives, take the initiative to overcome various learning difficulties, and constantly improve their interest in learning.

(2) to treat public courses, to recognize its practical value, and strive to indirect interest in public courses into direct learning interest.

(3) the study of elective courses, attention should be paid to only stay in the shallow understanding and understanding of the phenomenon.

(4) adjust the learning method.

after entering the university, the teacher-led teaching model has become a student-led self-learning model. teachers teach knowledge in the classroom, the students not only to digest the understanding of classroom learning content, but also a lot of reading the relevant books and literature. it can be said that the level of self-learning ability to become the most important factors affecting academic performance. in college, the content of teaching content, including more and more large, sitting alone in the classroom hard to read is difficult to adapt. we must learn to use modern high-tech teaching methods to master and enhance the knowledge learned. such as the internet, libraries, to get a lot of information to improve their ability. of course, college freshmen have to change some of the original concept: in the university, the test scores are not the most important indicators to measure people, people pay more attention to the comprehensive ability of the cultivation and overall quality improvement. here, the competition is potential, all-round.

interpersonal relations

communication is the most important part of interpersonal relationships, is between people to pass emotions, attitudes, facts, beliefs and ideas of the process, so good communication refers to a two-way communication process, not a person in speech, or play the other side to sing a one-man show, so in the study of life we should listen to each other\'s heart to say what? to understand each other thinking? the other side feel? and their own ideas back to each other. so i build good interpersonal relationships, we should start from the following aspects: the depth of self-awareness and acceptance; often sincere attitude; humble and gentle heart; moderate self-expression; respect and appreciate others; seek common values partner . 3 reasonable time arrangements

students learning time is limited, reasonable time, great significance. i feel that we should make full use of the study time during the day because of good mental state during the day, memory, active thinking, daytime learning efficiency is equivalent to one and a half hours of the night. every day before the class we are in the mind to do a simple learning plan, set yourself a small goal, to prevent unintended lectures. pre-school supplies ready to learn what to do a simple preview, focus on lectures in class. also, do not just focus on the whole time. second, to co-ordinate arrangements for extra-curricular learning time, to deal with things for the priorities, you can use the \"abc\" time classification, according to prioritized tasks are spanided into a (important), b (minor), c (general) three. important things to do first; secondary things, then deal with; flexible handling of the general things. in doing homework to adjust their state, as far as possible to make the brain, physical, emotional state in the best, the pursuit of higher efficiency.

4 linguistic aspects

in the university, we are from different places, because everyone\'s growth environment is so unreasonable to say so, how much slightly accent, so the new life in normal life and learning, should be more to the dictionary to learn good mandarin students learn to try to master the standard pronunciation. as a linguistic phenomenon applied to the public, mandarin is closely related to people \'s daily social life and is widely used in real life. so in order to better adapt to our society in the future, the time in the university should strive to improve their mandarin level.

5 continuous self-evaluation

correct self-evaluation is the condition that helps us to make the right direction of struggle, through two channels: direct self-evaluation and indirect self-evaluation. first of all, to recognize their own natural conditions, including health, mental state, emotional characteristics, interest, knowledge, professional expertise, intelligence, ability characteristics, and so on, followed by their own in different areas in practice to achieve the different results compared to find their own strengths, to determine the goal of struggle. indirect self-evaluation method, refers to the behavior of others and the contrast of the situation and found that the dislocation of self-knowledge.

time flies, in a blink of an eye we in the beautiful campus of agricultural university ushered in the sophomore of the second semester, each new start is a challenge, i believe that in this new semester, we can continue to challenge yourself, continuous progress, the pursuit of a more exciting life!

**测试员的自我评价篇七**

blink of an eye 10 years have gone, we ushered in a new year. summing up the work of the past year, from a personal point of view about the measurement of awareness.

quality is the life, quality is the fundamental guarantee for enterprise development. in the fierce competition in the construction market today, how to improve the construction quality management level is every enterprise managers must think about. factors affecting the quality of construction in all aspects. from the engineering measurement point of view, analyze the work of measuring the pay-off to ensure and improve the quality of the construction of an important role, and simply how to strengthen the management of measurement work to improve the quality of construction.

it is a very important technical work of municipal road engineering that the measuring and measuring line is an important technical work. it is inseparable from the whole process of construction, from the preparation before construction to the completion of the construction, to the final acceptance after construction. how to do a quick and good measurement of the line, is a basic technical skills and test the basic requirements.

do the measurement before the commencement of the end

before the start of the project, the survey and design units shall be responsible for on-site surveying and settlement according to the design documents, and the site standard point, conductor piles and crossing point piles shall be clearly identified according to the design drawings. within the measurement of signs, must take appropriate protection measures. on the measurement of the end, it is necessary to emphasize the protection of pile position, that is, in the design unit after pile, should be timely use of brick piers or pouring cement pier and other methods to be protected, so as not to lose. these piles are generally farmland or residential areas, it is easy to be man-made destruction, and once destroyed, let the survey and design units to fill test, then delay the construction, but also increase the cost.

midline retest and edge loft

center line measurement is based on the alignment measurement, the road center line plane position on the ground marked in detail. it is the difference with the alignment measurement is: alignment measurement, but the intersection of the road and the straight line segment of the necessary turning point marked out, and in the midline measurement, according to the intersection and the turning point with a series of stakes will road straight segment and curve segments are specified in detail on the ground.

the alignment survey is usually carried out by the survey and design units, and then the pile and measurement results to the construction side, the construction unit by the middle line and construction measurement.

subgrade construction should be fully restored before the center line, according to the restoration of the pile in the road and the relevant provisions of the roadbed side of the pile. on the midline re-measurement and edge lofting, should pay attention to the following points;

one should pay attention to the distance between the intersection, the direction is consistent with the drawings; such as an engineering project has several tenders, should pay attention to the center of the adjacent tenders are closed, midline measurements should be in-depth adjacent tenders 50 ~ 100 m; attention should be paid to the center of the structure such as bridge and culvert is closed; should pay attention to the relative position of the building and other buildings and drawings are consistent. if you find problems in a timely manner to identify the reasons for the design unit.

second, retaining pile set. it is very important to set up pile protection pile in the middle of the road, but these piles are easy to be destroyed during the construction. therefore, it is necessary to carry out the restoration and surveying work of the middle pile during the construction of the roadbed. in order to quickly and accurately restore the center pile in the original position, must be on the road before the construction of the main control point of the pile such as the intersection point, turning point, curve control points set up retaining pile. the so-called retaining pile, is outside the scope of the construction is not easy to be destroyed where some stakes set ing to these pile, with simple methods (such as the intersection point, range, etc.), you can quickly restore the original pile point.

set the pile should pay attention to the following aspects: in each straight section of the road, at least three control piles to set up retaining pile, so even if there is a control pile can not be restored, the other two points can be used to restore the straight section to the original position; the intersection angle of the two direction lines as close as possible to 90 °, should not be less than 30 ° angle of intersection; retaining pile should be selected outside the scope of construction, but not too far away; pile distance can not be too far; the retaining pile must be solid and reliable, pile to facilitate the erection of measuring instruments and observation.

set up retaining pile of curve side. for the curve segment, because of the more difficult to determine the side of the pile, re-measuring time-consuming more, so after a precise line, the edge of the curve section of the pile pile should also be set representative pile, which can reduce repeat the measurement, reducing the measurement workload.

third, the laying of mileage pile. after the midline pile is fixed, it is possible to lay out the control pile of the mileage pile on this basis. mileage pile layout principle is: in the straight section, generally arranged in every 100 meters of the entire pile of cross-section, similar to the common road construction 100 meters pile layout; in the curve section of the pile to be properly encrypted, in the curve mileage pile can be large stakes, above the mileage mark with paint or ink station, into the road outside the scope of construction on both sides of the ground, it is best to play on each side of a . to ensure that the construction is not easy to damage the case, from the embankment edge should be as close as possible to facilitate the use, generally 1 to 2 meters.

the laying of mileage piles is not addressed in most of the surveying and setting-out sections of the construction manual, and is not taken into account at many sites. i found in some sites, some construction technicians in the construction survey, the determination of the distance station is a long distance from a foot a foot row over, not only a waste of time and prone to cumulative error. if the mileage stakes are not allowed, then the elevation, slope quality control is out of the question.

third, the proofreading and additional standard point

first, the use of design units set up before the standard point should be carefully checked, close the gap may not exceed the limit, such as exceeding the allowable deviation should identify the reasons and promptly reported to the relevant departments. the design unit delivers the leveling points normally set several months ago. these points in the field can easily be man-made collision or natural subsidence due to the ground changes, so be sure to carefully review before use; second, the standard point of additional principles: the distance is generally 150 to 200 meters, plus transfer station for the principle. the additional standard point should be closed with the design unit to pay the standard point, such as an engineering project at several tenders, but also with the adjacent standard segment of the standard point of closure, the closure may not exceed the limit.

the position of the leveling point shall be located on a solid, non-sinking, non-touching ground or a solid building of a permanent building. can also be installed in the protection of deep-buried wood piles or concrete piles, and make clear signs. the leveling point should be checked once a month, and the level of the spot where the movement is suspected should be checked after re-inspection.

vertical and horizontal cross-section measurement

through the midline re-test, side piles line and the laying of the standard point, you can measure the vertical and horizontal cross-section. the main purpose of vertical and horizontal cross-section measurement is to calculate the amount of earth, so the vertical and horizontal cross-section measurement after the end of the measurement results should be checked with the design drawings. where the results with the original within the allowable deviation, the original results shall prevail, and only when there are significant differences with the original results, can be reported to the supervisory engineer after verification changes. it should be noted that: the work must be carried out before construction. if the measured amount of earth and the design does not conform to the supervision of the approval should also be carried out before site excavation to the supervisor before the actual amount of earthwork and design does not match, require additional visa, but the final supervision be sure to pay attention to the timeliness of the work.

本文档由站牛网zhann.net收集整理，更多优质范文文档请移步zhann.net站内查找